Encoder h261 [H.261]:
    General capabilities: none
    Threading capabilities: none
    Supported pixel formats: yuv420p
h261 encoder AVOptions:
  -mpv_flags         <flags>      E..V..... Flags common for all mpegvideo-based encoders. (default 0)
     skip_rd                      E..V..... RD optimal MB level residual skipping
     strict_gop                   E..V..... Strictly enforce gop size
     qp_rd                        E..V..... Use rate distortion optimization for qp selection
     cbp_rd                       E..V..... use rate distortion optimization for CBP
     naq                          E..V..... normalize adaptive quantization
     mv0                          E..V..... always try a mb with mv=<0,0>
  -luma_elim_threshold <int>        E..V..... single coefficient elimination threshold for luminance (negative values also consider dc coefficient) (from INT_MIN to INT_MAX) (default 0)
  -chroma_elim_threshold <int>        E..V..... single coefficient elimination threshold for chrominance (negative values also consider dc coefficient) (from INT_MIN to INT_MAX) (default 0)
  -quantizer_noise_shaping <int>        E..V..... (from 0 to INT_MAX) (default 0)
  -error_rate        <int>        E..V..... Simulate errors in the bitstream to test error concealment. (from 0 to INT_MAX) (default 0)
  -qsquish           <float>      E..V..... how to keep quantizer between qmin and qmax (0 = clip, 1 = use differentiable function) (from 0 to 99) (default 0)
  -rc_qmod_amp       <float>      E..V..... experimental quantizer modulation (from -FLT_MAX to FLT_MAX) (default 0)
  -rc_qmod_freq      <int>        E..V..... experimental quantizer modulation (from INT_MIN to INT_MAX) (default 0)
  -rc_eq             <string>     E..V..... Set rate control equation. When computing the expression, besides the standard functions defined in the section 'Expression Evaluation', the following functions are available: bits2qp(bits), qp2bits(qp). Also the following constants are available: iTex pTex tex mv fCode iCount mcVar var isI isP isB avgQP qComp avgIITex avgPITex avgPPTex avgBPTex avgTex.
  -rc_init_cplx      <float>      E..V..... initial complexity for 1-pass encoding (from -FLT_MAX to FLT_MAX) (default 0)
  -rc_buf_aggressivity <float>      E..V..... currently useless (from -FLT_MAX to FLT_MAX) (default 1)
  -border_mask       <float>      E..V..... increase the quantizer for macroblocks close to borders (from -FLT_MAX to FLT_MAX) (default 0)
  -lmin              <int>        E..V..... minimum Lagrange factor (VBR) (from 0 to INT_MAX) (default 236)
  -lmax              <int>        E..V..... maximum Lagrange factor (VBR) (from 0 to INT_MAX) (default 3658)
  -ibias             <int>        E..V..... intra quant bias (from INT_MIN to INT_MAX) (default 999999)
  -pbias             <int>        E..V..... inter quant bias (from INT_MIN to INT_MAX) (default 999999)
  -rc_strategy       <int>        E..V..... ratecontrol method (from 0 to 1) (default ffmpeg)
     ffmpeg          0            E..V..... deprecated, does nothing
     xvid            0            E..V..... deprecated, does nothing
  -motion_est        <int>        E..V..... motion estimation algorithm (from 0 to 2) (default epzs)
     zero            0            E..V.....
     epzs            1            E..V.....
     xone            2            E..V.....
  -force_duplicated_matrix <boolean>    E..V..... Always write luma and chroma matrix for mjpeg, useful for rtp streaming. (default false)
  -b_strategy        <int>        E..V..... Strategy to choose between I/P/B-frames (from 0 to 2) (default 0)
  -b_sensitivity     <int>        E..V..... Adjust sensitivity of b_frame_strategy 1 (from 1 to INT_MAX) (default 40)
  -brd_scale         <int>        E..V..... Downscale frames for dynamic B-frame decision (from 0 to 3) (default 0)
  -skip_threshold    <int>        E..V..... Frame skip threshold (from INT_MIN to INT_MAX) (default 0)
  -skip_factor       <int>        E..V..... Frame skip factor (from INT_MIN to INT_MAX) (default 0)
  -skip_exp          <int>        E..V..... Frame skip exponent (from INT_MIN to INT_MAX) (default 0)
  -skip_cmp          <int>        E..V..... Frame skip compare function (from INT_MIN to INT_MAX) (default dctmax)
     sad             0            E..V..... Sum of absolute differences, fast
     sse             1            E..V..... Sum of squared errors
     satd            2            E..V..... Sum of absolute Hadamard transformed differences
     dct             3            E..V..... Sum of absolute DCT transformed differences
     psnr            4            E..V..... Sum of squared quantization errors, low quality
     bit             5            E..V..... Number of bits needed for the block
     rd              6            E..V..... Rate distortion optimal, slow
     zero            7            E..V..... Zero
     vsad            8            E..V..... Sum of absolute vertical differences
     vsse            9            E..V..... Sum of squared vertical differences
     nsse            10           E..V..... Noise preserving sum of squared differences
     dct264          14           E..V.....
     dctmax          13           E..V.....
     chroma          256          E..V.....
     msad            15           E..V..... Sum of absolute differences, median predicted
  -sc_threshold      <int>        E..V..... Scene change threshold (from INT_MIN to INT_MAX) (default 0)
  -noise_reduction   <int>        E..V..... Noise reduction (from INT_MIN to INT_MAX) (default 0)
  -mpeg_quant        <int>        E..V..... Use MPEG quantizers instead of H.263 (from 0 to 1) (default 0)
  -ps                <int>        E..V..... RTP payload size in bytes (from INT_MIN to INT_MAX) (default 0)
  -mepc              <int>        E..V..... Motion estimation bitrate penalty compensation (1.0 = 256) (from INT_MIN to INT_MAX) (default 256)
  -mepre             <int>        E..V..... pre motion estimation (from INT_MIN to INT_MAX) (default 0)
  -a53cc             <boolean>    E..V..... Use A53 Closed Captions (if available) (default true)


