Decoder v210 [Uncompressed 4:2:2 10-bit]:
    General capabilities: dr1 
    Threading capabilities: none
V210 Decoder AVOptions:
  -custom_stride     <int>        .D.V..... Custom V210 stride (from INT_MIN to INT_MAX) (default 0)


