Demuxer s24le [PCM signed 24-bit little-endian]:
s24le demuxer AVOptions:
  -sample_rate       <int>        .D.......  (from 0 to INT_MAX) (default 44100)
  -channels          <int>        .D.......  (from 0 to INT_MAX) (default 1)


