Demuxer f32le [PCM 32-bit floating-point little-endian]:
f32le demuxer AVOptions:
  -sample_rate       <int>        .D.......  (from 0 to INT_MAX) (default 44100)
  -channels          <int>        .D.......  (from 0 to INT_MAX) (default 1)


