Filter limiter
  Limit pixels components to the specified range.
    slice threading supported
    Inputs:
       #0: default (video)
    Outputs:
       #0: default (video)
limiter AVOptions:
  min               <int>        ..FV..... set min value (from 0 to 65535) (default 0)
  max               <int>        ..FV..... set max value (from 0 to 65535) (default 65535)
  planes            <int>        ..FV..... set planes (from 0 to 15) (default 15)

This filter has support for timeline through the 'enable' option.

